Try mounting video mux to the top of the FM transmitter.

Try removing the modulator and PA and putting them in another enclosure.

Make faraday cage for mux.